


**Lab 3.2.1.9 – Configuring Basic RIPv2**

## Topology



**Objectives**

**Part 1: Build the Network and Configure Basic Device Settings**

**Part 2: Configure and Verify RIPv2 Routing**

* Configure RIPv2 on the routers and verify that it is running.
* Configure a passive interface.
* Examine routing tables.
* Disable automatic summarization.
* Configure a default route.
* Verify end-to-end connectivity.

**Addressing Table**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address** | **Subnet Mask** | **Default Gateway** |
| R1 | G0/0/1 | 172.30.10.1 | 255.255.255.0 | N/A |
|  | S0/1/0 (DCE) | 10.1.1.1 | 255.255.255.252 | N/A |
| R2 | G0/0/0 | 209.165.201.1 | 255.255.255.0 | N/A |
|  | S0/1/0 | 10.1.1.2 | 255.255.255.252 | N/A |
|  | S0/1/1 (DCE) | 10.2.2.2 | 255.255.255.252 | N/A |
| R3 | G0/0/1 | 172.30.30.1 | 255.255.255.0 | N/A |
|  | S0/1/1 | 10.2.2.1 | 255.255.255.252 | N/A |
| S1 | N/A | VLAN 1 | N/A | N/A |
| S3 | N/A | VLAN 1 | N/A | N/A |
| PC-A | NIC | 172.30.10.3 | 255.255.255.0 | 172.30.10.1 |
| PC-B | NIC | 209.165.201.2 | 255.255.255.0 | 209.165.201.1 |
| PC-C | NIC | 172.30.30.3 | 255.255.255.0 | 172.30.30.1 |

**Background / Scenario**

RIP version 2 (RIPv2) is used for routing of IPv4 addresses in small networks. RIPv2 is a classless, distance- vector routing protocol. Because RIPv2 is a classless routing protocol, subnet masks are included in the routing updates. By default, RIPv2 automatically summarizes networks at major network boundaries. When automatic summarization has been disabled, RIPv2 no longer summarizes networks to their classful address at boundary routers.

In this lab, you will configure the network topology with RIPv2 routing, disable automatic summarization, propagate a default route, and use CLI commands to display and verify RIP routing information.

**Part 1: Build the Network and Configure Basic Device Settings**

In Part 1, you will set up the network topology and configure basic settings.

**Step 1: Cable the network as shown in the topology. Step 2: Configure PC IP Addressing.**

Refer to the Addressing Table for IP address information of the PCs.

**Step 3: Configure basic settings for each router.**

Start **Tera Term** and click the **Serial** radio button. Verify that the **COM1** port is selected and click **OK** to continue. From the **Tera Term Setup** menu, choose the **Serial port** to verify the proper serial settings:

* Port: COM1
* Bits per second: 9600
* Data bits: 8
* Parity: None
* Stop bits: 1
* Flow Control: None

Would you like to enter the initial configuration dialog? [yes/no]: no

Press RETURN to get started!

**Router>**

1. Disable DNS lookup.
2. Configure device names as shown in the topology.
3. Configure password encryption.
4. Assign **class** as the privileged EXEC password.
5. Assign **cisco** as the console and vty passwords.
6. Configure a MOTD banner to warn users that unauthorized access is prohibited.
7. Configure **logging synchronous** for the console line.
8. Configure the IP addresses listed in the Addressing Table for all interfaces.
9. Configure a description for each interface with an IP address.
10. Configure the clock rate **128 000**, if applicable, to the **DCE** serial interface.

**Step 4: Test connectivity.**

At this point, the PCs are unable to ping each other.

1. Each workstation should be able to ping the attached router. Verify and troubleshoot if necessary.
2. The routers should be able to ping one another. Verify and troubleshoot if necessary.

|  |  |  |  |
| --- | --- | --- | --- |
| **From** | **To** | **IP Address (To)** | **Ping results** (Fail / Success) |
| **PC-A** | **R1 G0/0/1** | 172.30.10.1 |  |
| **PC-B** | **R2 G0/0/0** | 209.165.201.1 |  |
| **PC-C** | **R3 G0/0/1** | 172.30.30.1 |  |
| **R1** | **R2 S0/1/0** | 10.1.1.2 |  |
| **R3** | **R2 S0/1/1** | 10.2.2.2 |  |

**Part 2: Configure and Verify RIPv2 Routing**

In Part 2, you will configure RIPv2 routing on all routers in the network and then verify that the routing tables are updated correctly. After RIPv2 has been verified, you will disable automatic summarization, configure a default route, and verify end-to-end connectivity.

**Step 1: Configure RIPv2 routing.**

a. Configure **RIPv2** on **R1**as the routing protocol and advertise the appropriate connected networks.

R1# **config t**

R1(config)# **router rip**

R1(config-router)# **version 2**

R1(config-router)# **passive-interface g0/0/1**

R1(config-router)# **network 172.30.0.0**

R1(config-router)# **network 10.0.0.0**

The **passive-interface** command stops routing updates out the specified interface. This process prevents unnecessary routing traffic on the LAN. However, the network that the specified interface belongs to is still advertised in routing updates that are sent out across other interfaces.

1. Configure **RIPv2** on **R3** and use the **network** statement to add the appropriate connected networks and prevent routing updates on the LAN interface.
2. Configure **RIPv2** on **R2** and use the network statements to add the appropriate connected networks. Do not advertise the 209.165.201.0 network.

**Note**: It is not necessary to make the G0/0/0 interface passive on **R2** because the network associated with this interface is not being advertised.

**Step 2: Examine the current state of the network.**

* 1. The status of the two serial links can quickly be verified using the **show ip interface brief** command on R2.

#### R2# show ip interface brief

Interface IP-Address OK? Method Status Protocol Embedded-Service-Engine0/0 unassigned YES unset administratively down down GigabitEthernet0/0/0/0/0 209.165.201.1 YES manual up up GigabitEthernet0/0/0/0/1 unassigned YES unset administratively down down Serial0/1/0 10.1.1.2 YES manual up up

Serial0/1/1 10.2.2.2 YES manual up up

b. Check connectivity between PCs.

|  |
| --- |
| From PC-A, is it possible to ping PC-B? Why? |
| From PC-A, is it possible to ping PC-C? Why? |
| From PC-C, is it possible to ping PC-B? Why? |
| From PC-C, is it possible to ping PC-A? Why? |

1. Verify that RIPv2 is running on the routers.

You can use the **debug ip rip**, **show ip protocols**, and **show run** commands to confirm that RIPv2 is running. The **show ip protocols** command output for R1 is shown below.

#### R1# show ip protocols

Routing Protocol is "rip"

Outgoing update filter list for all interfaces is not set Incoming update filter list for all interfaces is not set Sending updates every 30 seconds, next due in 7 seconds Invalid after 180 seconds, hold down 180, flushed after 240 Redistributing: rip

Default version control: send version 2, receive 2

Interface Send Recv Triggered RIP Key-chain

Serial0/1/0 2 2

Automatic network summarization is in effect Maximum path: 4

Routing for Networks: 10.0.0.0

172.30.0.0

Passive Interface(s): GigabitEthernet0/0/0/0/1

Routing Information Sources:

|  |  |  |
| --- | --- | --- |
| Gateway | Distance | Last Update |
| 10.1.1.2 | 120 |  |

Distance: (default is 120)

|  |
| --- |
| When issuing the **debug ip rip** command on **R2**, what information is provided that confirms RIPv2 is running? **RIP: sending v2 updates to 224.0.0.9 via Serial 0/1/0 (10.1.1.2)** |
| When you are finished observing the debugging outputs, issue the **undebug all** command at the privileged EXEC prompt.  When issuing the **show run** command on **R3**, what information is provided that confirms RIPv2 is running? |
|  |

1. Examine the automatic summarization of routes.

The LANs connected to R1 and R3 are composed of discontiguous networks. R2 displays two equal-cost paths to the 172.30.0.0/16 network in the routing table. R2 displays only the major classful network address of 172.30.0.0 and does not display any of the subnets for this network.

R2# **show ip route**

<Output omitted>

10.0.0.0/8 is variably subnetted, 4 subnets, 2 masks C 10.1.1.0/30 is directly connected, Serial0/1/0

L 10.1.1.2/32 is directly connected, Serial0/1/0 C 10.2.2.0/30 is directly connected, Serial0/1/1 L 10.2.2.2/32 is directly connected, Serial0/1/1

R 172.30.0.0/16 [120/1] via 10.2.2.1, 00:00:23, Serial0/1/1

[120/1] via 10.1.1.1, 00:00:09, Serial0/1/0

209.165.201.0/24 is variably subnetted, 2 subnets, 2 masks

C 209.165.201.0/24 is directly connected, GigabitEthernet0/0/0/0 L 209.165.201.1/32 is directly connected, GigabitEthernet0/0/0/0

R1 displays only its own subnet for the 172.30.10.0/24 network. R1 does not have a route for the 172.30.30.0/24 subnet on R3.

R1# **show ip route**

<Output omitted>

10.0.0.0/8 is variably subnetted, 3 subnets, 2 masks C 10.1.1.0/30 is directly connected, Serial0/1/0

L 10.1.1.1/32 is directly connected, Serial0/1/0

R 10.2.2.0/30 [120/1] via 10.1.1.2, 00:00:21, Serial0/1/0

172.30.0.0/16 is variably subnetted, 2 subnets, 2 masks

C 172.30.10.0/24 is directly connected, GigabitEthernet0/0/1 L 172.30.10.1/32 is directly connected, GigabitEthernet0/0/1

**R3** only displays its own subnet for the 172.30.30.0/24 network. R3 does not have a route for the 172.30.10.0/24 subnets on R1.

R3# **show ip route**

10.0.0.0/8 is variably subnetted, 3 subnets, 2 masks C 10.2.2.0/30 is directly connected, Serial0/1/1

L 10.2.2.1/32 is directly connected, Serial0/1/1

R 10.1.1.0/30 [120/1] via 10.2.2.2, 00:00:23, Serial0/1/1

172.30.0.0/16 is variably subnetted, 2 subnets, 2 masks

C 172.30.30.0/24 is directly connected, GigabitEthernet0/0/1 L 172.30.30.1/32 is directly connected, GigabitEthernet0/0/1

Use the **debug ip rip** command on **R2** to determine the routes received in the RIP updates from R3 and

list them here. **R2#unRIP: received v2 update from 10.2.2.1 on Serial0/1/1**

R3 is not sending any of the 172.30.0.0 subnets, only the summarized route of 172.30.0.0/16, including

the subnet mask. Therefore, the routing tables on R1 and R2 do not display the 172.30.0.0 subnets on R3.

**Step 3: Disable automatic summarization.**

a. The **no auto-summary** command is used to turn off automatic summarization in RIPv2. Disable auto summarization on **all routers**. The routers will no longer summarize routes at major classful network boundaries. **R1** is shown here as an example.

R1(config)# **router rip**

R1(config-router)# **no auto-summary**

b. Issue the **clear ip route \*** command to clear the routing table. **To be effective, execute this command at least three times.**

R1(config-router)# **end**

R1# **clear ip route \***

c. Examine the routing tables. Remember that it will take some time to converge the routing tables after clearing them.

The LAN subnets connected to R1 and R3 should now be included in all three routing tables.

R2# **show ip route**

ateway of last resort is not set

10.0.0.0/8 is variably subnetted, 4 subnets, 2 masks

C 10.1.1.0/30 is directly connected, Serial0/1/0 L 10.1.1.2/32 is directly connected, Serial0/1/0 C 10.2.2.0/30 is directly connected, Serial0/1/1 L 10.2.2.2/32 is directly connected, Serial0/1/1

172.30.0.0/16 is variably subnetted, 3 subnets, 2 masks

R 172.30.0.0/16 [120/1] via 10.2.2.1, 00:01:01, Serial0/1/1

[120/1] via 10.1.1.1, 00:01:15, Serial0/1/0 R 172.30.10.0/24 [120/1] via 10.1.1.1, 00:00:21, Serial0/1/0 R 172.30.30.0/24 [120/1] via 10.2.2.1, 00:00:04, Serial0/1/1

209.165.201.0/24 is variably subnetted, 2 subnets, 2 masks

C 209.165.201.0/24 is directly connected, GigabitEthernet0/0/0/0 L 209.165.201.1/32 is directly connected, GigabitEthernet0/0/0/0

R1# **show ip route**

<Output omitted>

Gateway of last resort is not set

10.0.0.0/8 is variably subnetted, 3 subnets, 2 masks C 10.1.1.0/30 is directly connected, Serial0/1/0

L 10.1.1.1/32 is directly connected, Serial0/1/0

R 10.2.2.0/30 [120/1] via 10.1.1.2, 00:00:12, Serial0/1/0

172.30.0.0/16 is variably subnetted, 3 subnets, 2 masks

C 172.30.10.0/24 is directly connected, GigabitEthernet0/0/1 L 172.30.10.1/32 is directly connected, GigabitEthernet0/0/1

R 172.30.30.0/24 [120/2] via 10.1.1.2, 00:00:12, Serial0/1/0

R3# **show ip route**

<Output omitted>

10.0.0.0/8 is variably subnetted, 3 subnets, 2 masks C 10.2.2.0/30 is directly connected, Serial0/1/1

L 10.2.2.1/32 is directly connected, Serial0/1/1

R 10.1.1.0/30 [120/1] via 10.2.2.2, 00:00:23, Serial0/1/1

172.30.0.0/16 is variably subnetted, 2 subnets, 2 masks

C 172.30.30.0/24 is directly connected, GigabitEthernet0/0/1 L 172.30.30.1/32 is directly connected, GigabitEthernet0/0/1 R 172.30.10.0 [120/2] via 10.2.2.2, 00:00:16, Serial0/1/1

**Step 4: Configure and redistribute a default route for Internet access.**

a. From R2, create a static route to network 0.0.0.0 0.0.0.0, using the **ip route** command. This forwards any traffic with an unknown destination address to PC-B at 209.165.201.2, simulating the Internet by setting a Gateway of Last Resort on router R2.

R2(config)# **ip route 0.0.0.0 0.0.0.0 209.165.201.2**

b. R2 will advertise a route to the other routers if the **default-information originate** command is added to its RIP configuration.

R2(config)# **router rip**

R2(config-router)# **default-information originate**

### Step 5: Verify the routing configuration.

1. View the routing table on R1.

R1# **show ip route**

<Output omitted>

Gateway of last resort is 10.1.1.2 to network 0.0.0.0

R\* 0.0.0.0/0 [120/1] via 10.1.1.2, 00:00:13, Serial0/1/0

10.0.0.0/8 is variably subnetted, 3 subnets, 2 masks C 10.1.1.0/30 is directly connected, Serial0/1/0

L 10.1.1.1/32 is directly connected, Serial0/1/0

R 10.2.2.0/30 [120/1] via 10.1.1.2, 00:00:13, Serial0/1/0

172.30.0.0/16 is variably subnetted, 3 subnets, 2 masks

C 172.30.10.0/24 is directly connected, GigabitEthernet0/0/1 L 172.30.10.1/32 is directly connected, GigabitEthernet0/0/1

R 172.30.30.0/24 [120/2] via 10.1.1.2, 00:00:13, Serial0/1/0

How can you tell from the routing table that the subnetted network shared by R1 and R3 has a pathway for Internet traffic?

1. View the routing table on R2.

How is the pathway for Internet traffic provided in its routing table?

**Step 6: Verify connectivity.**

a. Simulate sending traffic to the Internet by pinging from PC-A and PC-C to 209.165.201.2.

Were the pings successful?

b. Verify that hosts within the subnetted network can reach each other by pinging between PC-A and PC-C.

Were the pings successful?

**Note**: It may be necessary to disable the PCs firewall.

**Reflection**

1. Why would you turn off automatic summarization for RIPv2?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. How did R1 and R3 learn the pathway to the Internet?