


**Lab 9.2.2.6 – Configuring Dynamic and Static NAT**



**Addressing Table**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address** | **Subnet Mask** | **Default Gateway** |
| Gateway | G0/1 | 192.168.1.1 | 255.255.255.0 | N/A |
|  | S0/1/1 | 209.165.201.18 | 255.255.255.252 | N/A |
| ISP | S0/1/0 (DCE) | 209.165.201.17 | 255.255.255.252 | N/A |
|  | Lo0 | 192.31.7.1 | 255.255.255.255 | N/A |
| PC-A (Simulated Server) | NIC | 192.168.1.20 | 255.255.255.0 | 192.168.1.1 |
| PC-B | NIC | 192.168.1.21 | 255.255.255.0 | 192.168.1.1 |

**Objectives**

#### Part 1: Build the Network and Verify Connectivity Part 2: Configure and Verify Static NAT

**Part 3: Configure and Verify Dynamic NAT**

**Background / Scenario**

Network Address Translation (NAT) is the process where a network device, such as a Cisco router, assigns a **public address** to host devices inside a **private network**. The main reason to use NAT is to reduce the number of public IP addresses that an organization uses because the number of available IPv4 public addresses is limited. In this lab, an ISP has allocated the public IP address space of **209.165.200.224/27** to a company. This provides the company with 30 public IP addresses. The addresses, **209.165.200.225 to 209.165.200.241**, are for static allocation and **209.165.200.242 to 209.165.200.254** are for dynamic allocation. A static route is used from the ISP to the gateway router, and a default route is used from the gateway to the ISP router. The ISP connection to the Internet is simulated by a loopback address on the ISP router.

# Part 1: Build the Network and Verify Connectivity

In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, static routing, device access, and passwords.

* 1. Configure PC hosts.
  2. Configure basic settings for each router.
     1. Console into the router and enter global configuration mode.
     2. Copy the following basic configuration and paste it to the running-configuration on the router.

no ip domain-lookup

service password-encryption

enable secret class

banner motd #

Unauthorized access is strictly prohibited. #

line con 0

password cisco

login

logging synchronous

line vty 0 4

password cisco

login

* + 1. Configure the host name as shown in the topology.
    2. Configure the IPv4 addresses on the router as shown in the topology.
    3. Set the DCE serial interfaces with a clock rate of **128000**.
  1. Configure static routing.
     1. Create a static route from the ISP router to the Gateway router using the assigned public network address range **209.165.200.224/27**.

ISP(config)# **ip route 209.165.200.224 255.255.255.224 209.165.201.18**

* + 1. Create a default route from the Gateway router to the ISP router.

Gateway(config)# **ip route 0.0.0.0 0.0.0.0 209.165.201.17**

* 1. Verify network connectivity.
     1. From the **PC-A** and **PC-B**, **ping** the **G0/1** interface on the **Gateway** router. Troubleshoot if the pings are unsuccessful.

|  |  |  |  |
| --- | --- | --- | --- |
| **From** | **To** | **IP Address (To)** | **Ping results** (Fail / Success) |
| **PC-A** | **Gateway G0/1** | **192.168.1.1** |  |
| **PC-B** | **Gateway G0/1** | **192.168.1.1** |  |

* + 1. Display the routing tables (**sh ip route**) on both routers to verify that the static routes are in the routing table and configured correctly on both routers.

# Part 2: Configure and Verify Static NAT

Static NAT uses a one-to-one mapping of local and global addresses, and these mappings remain constant. Static NAT is particularly useful for web servers or devices that must have static addresses that are accessible from the Internet.

* 1. Configure a static mapping.

A static map is configured to tell the router to translate between the private inside server address **192.168.1.20** and the public address **209.165.200.225**. This allows a user from the Internet to access PC-A. PC-A is simulating a server or device with a constant address that can be accessed from the Internet.

Gateway(config)# **ip nat inside source static 192.168.1.20 209.165.200.225**

* 1. Specify the interfaces.

Issue the **ip nat inside** and **ip nat outside** commands to the interfaces.

Gateway(config)# **interface g0/1**

Gateway(config-if)# **ip nat inside**

Gateway(config-if)# **interface s0/1/1**

Gateway(config-if)# **ip nat outside**

* 1. Test the configuration.
     1. Display the static NAT table by issuing the **show ip nat translations** command.

Gateway# **show ip nat translations**

Pro Inside global Inside local Outside local Outside global

--- 209.165.200.225 192.168.1.20 --- ---

What is the translation of the Inside local host address?

192.168.1.20 = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The Inside global address is assigned by?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The Inside local address is assigned by?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. From **PC-A**, **ping** the **Lo0** interface **(192.31.7.1)** on **ISP**. If the ping was unsuccessful, troubleshoot and correct the issues. On the Gateway router, display the NAT table.

Gateway# **show ip nat translations**

Pro Inside global Inside local Outside local Outside global

icmp 209.165.200.225:5 192.168.1.20:5 192.31.7.1:5 192.31.7.1:5

icmp 209.165.200.225:6 192.168.1.20:6 192.31.7.1:6 192.31.7.1:6

icmp 209.165.200.225:7 192.168.1.20:7 192.31.7.1:7 192.31.7.1:7

icmp 209.165.200.225:8 192.168.1.20:8 192.31.7.1:8 192.31.7.1:8

--- 209.165.200.225 192.168.1.20 --- ---

A NAT entry was added to the table with ICMP listed as the protocol when **PC-A** sent an ICMP request (ping) to **192.31.7.1** on ISP.

What port numbers were used in this ICMP exchange? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. From **PC-A**, **telnet** to the **ISP Lo0** (**192.31.7.1**). On the Gateway router, display the NAT table.

Gateway# **show ip nat translations**

Pro Inside global Inside local Outside local Outside global

--- 209.165.200.225 192.168.1.20 --- ---

tcp 209.165.200.225:1025 192.168.1.20:1025 192.31.7.1:23 192.31.7.1:23

**Note**: The NAT for the ICMP request may have timed out and been removed from the NAT table.

What was the protocol used in this translation? \_\_\_\_\_\_\_\_\_\_\_\_

What are the port numbers used?

Inside global / local: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Outside global / local: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Because static NAT was configured for **PC-A**, verify that pinging from **ISP** to **PC-A** at the static NAT public address **(209.165.200.225)** is successful.
    2. On the Gateway router, display the NAT table to verify the translation.

Gateway# **show ip nat translations**

Pro Inside global Inside local Outside local Outside global

icmp 209.165.200.225:1 192.168.1.20:1 209.165.201.17:1 209.165.201.17:1

icmp 209.165.200.225:2 192.168.1.20:2 209.165.201.17:2 209.165.201.17:2

icmp 209.165.200.225:3 192.168.1.20:3 209.165.201.17:3 209.165.201.17:3

icmp 209.165.200.225:4 192.168.1.20:4 209.165.201.17:4 209.165.201.17:4

icmp 209.165.200.225:5 192.168.1.20:5 209.165.201.17:5 209.165.201.17:5

--- 209.165.200.225 192.168.1.20 --- ---

tcp 209.165.200.225:1025 192.168.1.20:1025 192.31.7.1:23 192.31.7.1:23

Notice that the Outside local and Outside global addresses are the same. This address is the ISP remote network source address. For the ping from the ISP to succeed, the Inside global static NAT address 209.165.200.225 was translated to the Inside local address of PC-A (192.168.1.20).

* + 1. Verify NAT statistics by using the **show ip nat statistics** command on the Gateway router.

Gateway# **show ip nat statistics**

Total translations: 7 (1 static, 6 dynamic, 6 extended)

Outside Interfaces: Serial0/1/1

Inside Interfaces: GigabitEthernet0/1

Hits: 74 Misses: 10

Expired translations: 4

Dynamic mappings:

**Note**: This is only a sample output. Your output may not match exactly.

# Part 3: Configure and Verify Dynamic NAT

Dynamic NAT uses a pool of public addresses and assigns them on a first-come, first-served basis. When an inside device requests access to an outside network, dynamic NAT assigns an available public IPv4 address from the pool. Dynamic NAT results in a many-to-many address mapping between local and global addresses.

### Step 1: Clear NATs.

Before proceeding to add dynamic NATs, clear the NATs and statistics from Part 2.

Gateway# **clear ip nat translation \***

### Step 2: Define an access control list (ACL) that matches the LAN private IP address range.

ACL 1 is used to allow 192.168.1.0/24 network to be translated.

Gateway(config)# **access-list 1 permit 192.168.1.0 0.0.0.255**

### Step 3: Verify that the NAT interface configurations are still valid.

Issue the **show ip nat statistics** command on the **Gateway** router to verify the NAT configurations.

Total translations: 1 (1 static, 0 dynamic, 0 extended)

Outside Interfaces: Serial0/1/1

Inside Interfaces: GigabitEthernet0/1

Hits: 77 Misses: 10

Expired translations: 9

Dynamic mappings:

### Step 4: Define the pool of usable public IP addresses.

Gateway(config)# **ip nat pool public\_access 209.165.200.242 209.165.200.254 netmask 255.255.255.224**

**Step 5: Define the NAT from the inside source list to the outside pool.**

**Note**: Remember that NAT pool names are case-sensitive and the pool name entered here must match that used in the previous step.

Gateway(config)# **ip nat inside source list 1 pool public\_access**

**Step 6: Test the configuration.**

1. From **PC-B**, ping the **Lo0** interface (**192.31.7.1**) on **ISP**. If the ping was unsuccessful, troubleshoot and correct the issues. On the **Gateway** router, display the NAT table.

Gateway# **show ip nat translations**

Pro Inside global Inside local Outside local Outside global

icmp 209.165.200.242:5 192.168.1.21:5 192.31.7.1:5 192.31.7.1:5

icmp 209.165.200.242:6 192.168.1.21:6 192.31.7.1:6 192.31.7.1:6

icmp 209.165.200.242:7 192.168.1.21:7 192.31.7.1:7 192.31.7.1:7

icmp 209.165.200.242:8 192.168.1.21:8 192.31.7.1:8 192.31.7.1:8

--- 209.165.200.225 192.168.1.20 --- ---

What is the translation of the Inside local host address for **PC-B**?

192.168.1.21 = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

A dynamic NAT entry was added to the table with ICMP as the protocol when **PC-B** sent an ICMP message to **192.31.7.1** on **ISP**.

What port numbers were used in this ICMP exchange? \_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Verify NAT statistics by using the **show ip nat statistics** command on the Gateway router.

Gateway# **show ip nat statistics**

Total translations: 1 (1 static, 0 dynamic, 0 extended)

Outside Interfaces: Serial0/1/1

Inside Interfaces: GigabitEthernet0/1

Hits: 81 Misses: 14

Expired translations: 13

Dynamic mappings:

-- Inside Source

access-list 1 pool public\_access refCount 0

pool public\_access: netmask 255.255.255.224

start 209.165.200.242 end 209.165.200.254

type generic, total addresses 13 , allocated 0 (0%), misses 0

**Note**: This is only a sample output. Your output may not match exactly.

* 1. Remove the static NAT entry.

In Step 7, the static NAT entry is removed and you can observe the NAT entry.

* + 1. Remove the **static NAT** from Part 2. Enter **yes** when prompted to delete child entries.

Gateway(config)# **no ip nat inside source static 192.168.1.20 209.165.200.225**

Static entry in use, do you want to delete child entries? [no]: **yes**

* + 1. Clear the NATs and statistics.

Gateway# **clear ip nat translation \***

* + 1. Ping the **ISP (192.31.7.1)** from both hosts.

|  |  |  |  |
| --- | --- | --- | --- |
| **From** | **To** | **IP Address (To)** | **Ping results** (Fail / Success) |
| **PC-A** | **ISP Lo0** | **192.31.7.1** |  |
| **PC-B** | **ISP Lo0** | **192.31.7.1** |  |

* + 1. Display the NAT table and statistics.

Gateway# **show ip nat translation**

Pro Inside global Inside local Outside local Outside global

icmp 209.165.200.243:13 192.168.1.20:13 192.31.7.1:13 192.31.7.1:13

icmp 209.165.200.243:14 192.168.1.20:14 192.31.7.1:14 192.31.7.1:14

icmp 209.165.200.243:15 192.168.1.20:15 192.31.7.1:15 192.31.7.1:15

icmp 209.165.200.243:16 192.168.1.20:16 192.31.7.1:16 192.31.7.1:16

icmp 209.165.200.244:13 192.168.1.21:13 192.31.7.1:13 192.31.7.1:13

icmp 209.165.200.244:14 192.168.1.21:14 192.31.7.1:14 192.31.7.1:14

icmp 209.165.200.244:15 192.168.1.21:15 192.31.7.1:15 192.31.7.1:15

icmp 209.165.200.244:16 192.168.1.21:16 192.31.7.1:16 192.31.7.1:16

**Note**: This is only a sample output. Your output may not match exactly.

Gateway# **show ip nat statistics**

Total translations: 8 (0 static, 8 dynamic, 8 extended)

Outside Interfaces: Serial0/1/1

Inside Interfaces: GigabitEthernet0/1

Hits: 97 Misses: 30

Expired translations: 21

Dynamic mappings:

-- Inside Source

access-list 1 pool public\_access refCount 8

pool public\_access: netmask 255.255.255.224

start 209.165.200.242 end 209.165.200.254

type generic, total addresses 13 , allocated 2 (15%), misses 0

1. Reflection
   1. Why would NAT be used in a network?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_