**!---------------------------------------------**

**! Router WEST**

**!---------------------------------------------**

**en**

**config t**

**hostname WEST**

**no ip domain-lookup**

**service password-encryption**

**enable secret class**

**banner motd #Unauthorized access is strictly prohibited#**

**line con 0**

**password cisco**

**login**

**logging synchronous**

**exit**

**line vty 0 4**

**password cisco**

**login**

**exit**

**interface tunnel 0**

**tunnel source Serial0/1/0**

**tunnel destination 10.2.2.1**

**ip address 172.16.12.1 255.255.255.252**

**exit**

**interface GigabitEthernet0/0/1**

**ip address 172.16.1.1 255.255.255.0**

**no shut**

**exit**

**interface Serial0/1/0**

**ip address 10.1.1.1 255.255.255.252**

**clock rate 64000**

**no shut**

**exit**

**router ospf 1**

**network 172.16.1.0 0.0.0.255 area 0**

**network 172.16.12.0 0.0.0.3 area 0**

**exit**

**ip route 0.0.0.0 0.0.0.0 10.1.1.2**

**!---------------------------------------------**

**! Router EAST**

**!---------------------------------------------**

**en**

**config t**

**hostname EAST**

**no ip domain-lookup**

**service password-encryption**

**enable secret class**

**banner motd #Unauthorized access is strictly prohibited#**

**line con 0**

**password cisco**

**login**

**logging synchronous**

**exit**

**line vty 0 4**

**password cisco**

**login**

**exit**

**interface tunnel 0**

**tunnel source Serial0/1/1**

**tunnel destination 10.1.1.1**

**ip address 172.16.12.2 255.255.255.252**

**exit**

**interface G0/0/1**

**ip address 172.16.2.1 255.255.255.0**

**no shut**

**exit**

**interface Serial0/1/1**

**ip address 10.2.2.1 255.255.255.252**

**no shut**

**exit**

**router ospf 1**

**network 172.16.2.0 0.0.0.255 area 0**

**network 172.16.12.0 0.0.0.3 area 0**

**exit**

**ip route 0.0.0.0 0.0.0.0 10.2.2.2**

**!---------------------------------------------**

**! Router ISP**

**!---------------------------------------------**

**en**

**config t**

**hostname ISP**

**no ip domain-lookup**

**service password-encryption**

**enable secret class**

**banner motd #Unauthorized access is strictly prohibited#**

**line con 0**

**password cisco**

**login**

**logging synchronous**

**exit**

**line vty 0 4**

**password cisco**

**login**

**exit**

**interface Serial0/1/0**

**ip address 10.1.1.2 255.255.255.252**

**no shut**

**exit**

**interface Serial0/1/1**

**ip address 10.2.2.2 255.255.255.252**

**clock rate 64000**

**no shut**

**exit**